CoinUtils 2.10.15

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Friends Macros Groups Pages
List of all members
CoinMpsCardReader Class Reference

Very simple code for reading MPS data. More...

`#include <CoinMpsIO.hpp>`

Collaboration diagram for CoinMpsCardReader:
[legend]

## Public Member Functions
Constructor and destructor
| CoinMpsCardReader (CoinFileInput *input, CoinMpsIO *reader)
| Constructor expects file to be open This one takes gzFile if fp null. More...
| ~CoinMpsCardReader ()
| Destructor. More...
card stuff
COINSectionType | readToNextSection ()
| Read to next section. More...
COINSectionType | nextField ()
| Gets next field and returns section type e.g. COIN_COLUMN_SECTION. More...
int | nextGmsField (int expectedType)
| Gets next field for .gms file and returns type. More...
COINSectionType | whichSection () const
| Returns current section type. More...
void | setWhichSection (COINSectionType section)
| Sets current section type. More...
bool | freeFormat () const
| Sees if free format. More...
void | setFreeFormat (bool yesNo)
| Sets whether free format. Mainly for blank RHS etc. More...
COINMpsType | mpsType () const
| Only for first field on card otherwise BLANK_COLUMN e.g. More...
int | cleanCard ()
| Reads and cleans card - taking out trailing blanks - return 1 if EOF. More...
const char * | rowName () const
| Returns row name of current field. More...
const char * | columnName () const
| Returns column name of current field. More...
double | value () const
| Returns value in current field. More...
const char * | valueString () const
| Returns value as string in current field. More...
const char * | card () const
| Whole card (for printing) More...
char * | mutableCard ()
| Whole card - so we look at it (not const so nextBlankOr will work for gms reader) More...
void | setPosition (char *position)
| set position (again so gms reader will work) More...
char * | getPosition () const
| get position (again so gms reader will work) More...
CoinBigIndex | cardNumber () const
| Returns card number. More...
CoinFileInput * | fileInput () const
| Returns file input. More...
void | setStringsAllowed ()
| Sets whether strings allowed. More...

## Protected Attributes
data
double | value_
| Current value. More...
char | card_ [MAX_CARD_LENGTH]
| Current card image. More...
char * | position_
| Current position within card image. More...
char * | eol_
| End of card. More...
COINMpsType | mpsType_
| Current COINMpsType. More...
char | rowName_ [COIN_MAX_FIELD_LENGTH]
| Current row name. More...
char | columnName_ [COIN_MAX_FIELD_LENGTH]
| Current column name. More...
CoinFileInput * | input_
| File input. More...
COINSectionType | section_
| Which section we think we are in. More...
CoinBigIndex | cardNumber_
| Card number. More...
bool | freeFormat_
| Whether free format. Just for blank RHS etc. More...
int | ieeeFormat_
| Whether IEEE - 0 no, 1 INTEL, 2 not INTEL. More...
bool | eightChar_
| If all names <= 8 characters then allow embedded blanks. More...
CoinMpsIO * | reader_
| MpsIO. More...
CoinMessageHandler * | handler_
| Message handler. More...
CoinMessages | messages_
| Messages. More...
char | valueString_ [COIN_MAX_FIELD_LENGTH]
| Current element as characters (only if strings allowed) More...
bool | stringsAllowed_
| Whether strings allowed. More...

## methods
double | osi_strtod (char *ptr, char **output, int type)
| type - 0 normal, 1 INTEL IEEE, 2 other IEEE More...
double | osi_strtod (char *ptr, char **output)
| For strings. More...
static void | strcpyAndCompress (char *to, const char *from)
| remove blanks More...
static char * | nextBlankOr (char *image)

## Detailed Description

Very simple code for reading MPS data.

Definition at line 59 of file CoinMpsIO.hpp.

## Constructor & Destructor Documentation

CoinMpsCardReader::CoinMpsCardReader | ( | CoinFileInput * | input,
|  | CoinMpsIO * | reader
| ) |  |

Constructor expects file to be open This one takes gzFile if fp null.

CoinMpsCardReader::~CoinMpsCardReader | ( |  | ) |

Destructor.

## Member Function Documentation

COINSectionType CoinMpsCardReader::readToNextSection | ( |  | ) |

Read to next section.

COINSectionType CoinMpsCardReader::nextField | ( |  | ) |

Gets next field and returns section type e.g. COIN_COLUMN_SECTION.

int CoinMpsCardReader::nextGmsField | ( | int | expectedType | ) |

Gets next field for .gms file and returns type.

-1 - EOF 0 - what we expected (and processed so pointer moves past) 1 - not what we expected leading blanks always ignored input types 0 - anything - stops on non blank card 1 - name (in columnname) 2 - value 3 - value name pair 4 - equation type 5 - ;

COINSectionType CoinMpsCardReader::whichSection | ( |  | ) | const
| inline

Returns current section type.

Definition at line 95 of file CoinMpsIO.hpp.

void CoinMpsCardReader::setWhichSection | ( | COINSectionType | section | ) |
| inline

Sets current section type.

Definition at line 99 of file CoinMpsIO.hpp.

bool CoinMpsCardReader::freeFormat | ( |  | ) | const
| inline

Sees if free format.

Definition at line 103 of file CoinMpsIO.hpp.

void CoinMpsCardReader::setFreeFormat | ( | bool | yesNo | ) |
| inline

Sets whether free format. Mainly for blank RHS etc.

Definition at line 106 of file CoinMpsIO.hpp.

COINMpsType CoinMpsCardReader::mpsType | ( |  | ) | const
| inline

Only for first field on card otherwise BLANK_COLUMN e.g.

COIN_E_ROW

Definition at line 110 of file CoinMpsIO.hpp.

int CoinMpsCardReader::cleanCard | ( |  | ) |

Reads and cleans card - taking out trailing blanks - return 1 if EOF.

const char* CoinMpsCardReader::rowName | ( |  | ) | const
| inline

Returns row name of current field.

Definition at line 116 of file CoinMpsIO.hpp.

const char* CoinMpsCardReader::columnName | ( |  | ) | const
| inline

Returns column name of current field.

Definition at line 120 of file CoinMpsIO.hpp.

double CoinMpsCardReader::value | ( |  | ) | const
| inline

Returns value in current field.

Definition at line 124 of file CoinMpsIO.hpp.

const char* CoinMpsCardReader::valueString | ( |  | ) | const
| inline

Returns value as string in current field.

Definition at line 128 of file CoinMpsIO.hpp.

const char* CoinMpsCardReader::card | ( |  | ) | const
| inline

Whole card (for printing)

Definition at line 132 of file CoinMpsIO.hpp.

char* CoinMpsCardReader::mutableCard | ( |  | ) |
| inline

Whole card - so we look at it (not const so nextBlankOr will work for gms reader)

Definition at line 136 of file CoinMpsIO.hpp.

void CoinMpsCardReader::setPosition | ( | char * | position | ) |
| inline

set position (again so gms reader will work)

Definition at line 140 of file CoinMpsIO.hpp.

char* CoinMpsCardReader::getPosition | ( |  | ) | const
| inline

get position (again so gms reader will work)

Definition at line 143 of file CoinMpsIO.hpp.

CoinBigIndex CoinMpsCardReader::cardNumber | ( |  | ) | const
| inline

Returns card number.

Definition at line 146 of file CoinMpsIO.hpp.

CoinFileInput* CoinMpsCardReader::fileInput | ( |  | ) | const
| inline

Returns file input.

Definition at line 150 of file CoinMpsIO.hpp.

void CoinMpsCardReader::setStringsAllowed | ( |  | ) |
| inline

Sets whether strings allowed.

Definition at line 154 of file CoinMpsIO.hpp.

double CoinMpsCardReader::osi_strtod | ( | char * | ptr,
|  | char ** | output,
|  | int | type
| ) |  |

type - 0 normal, 1 INTEL IEEE, 2 other IEEE

static void CoinMpsCardReader::strcpyAndCompress | ( | char * | to,
|  | const char * | from
| ) |  |
| static

remove blanks

static char* CoinMpsCardReader::nextBlankOr | ( | char * | image | ) |
| static

double CoinMpsCardReader::osi_strtod | ( | char * | ptr,
|  | char ** | output
| ) |  |

For strings.

## Member Data Documentation

double CoinMpsCardReader::value_
| protected

Current value.

Definition at line 164 of file CoinMpsIO.hpp.

char CoinMpsCardReader::card_[MAX_CARD_LENGTH]
| protected

Current card image.

Definition at line 166 of file CoinMpsIO.hpp.

char* CoinMpsCardReader::position_
| protected

Current position within card image.

Definition at line 168 of file CoinMpsIO.hpp.

char* CoinMpsCardReader::eol_
| protected

End of card.

Definition at line 170 of file CoinMpsIO.hpp.

COINMpsType CoinMpsCardReader::mpsType_
| protected

Current COINMpsType.

Definition at line 172 of file CoinMpsIO.hpp.

char CoinMpsCardReader::rowName_[COIN_MAX_FIELD_LENGTH]
| protected

Current row name.

Definition at line 174 of file CoinMpsIO.hpp.

char CoinMpsCardReader::columnName_[COIN_MAX_FIELD_LENGTH]
| protected

Current column name.

Definition at line 176 of file CoinMpsIO.hpp.

CoinFileInput* CoinMpsCardReader::input_
| protected

File input.

Definition at line 178 of file CoinMpsIO.hpp.

COINSectionType CoinMpsCardReader::section_
| protected

Which section we think we are in.

Definition at line 180 of file CoinMpsIO.hpp.

CoinBigIndex CoinMpsCardReader::cardNumber_
| protected

Card number.

Definition at line 182 of file CoinMpsIO.hpp.

bool CoinMpsCardReader::freeFormat_
| protected

Whether free format. Just for blank RHS etc.

Definition at line 184 of file CoinMpsIO.hpp.

int CoinMpsCardReader::ieeeFormat_
| protected

Whether IEEE - 0 no, 1 INTEL, 2 not INTEL.

Definition at line 186 of file CoinMpsIO.hpp.

bool CoinMpsCardReader::eightChar_
| protected

If all names <= 8 characters then allow embedded blanks.

Definition at line 188 of file CoinMpsIO.hpp.

CoinMpsIO* CoinMpsCardReader::reader_
| protected

MpsIO.

Definition at line 190 of file CoinMpsIO.hpp.

CoinMessageHandler* CoinMpsCardReader::handler_
| protected

Message handler.

Definition at line 192 of file CoinMpsIO.hpp.

CoinMessages CoinMpsCardReader::messages_
| protected

Messages.

Definition at line 194 of file CoinMpsIO.hpp.

char CoinMpsCardReader::valueString_[COIN_MAX_FIELD_LENGTH]
| protected

Current element as characters (only if strings allowed)

Definition at line 196 of file CoinMpsIO.hpp.

bool CoinMpsCardReader::stringsAllowed_
| protected

Whether strings allowed.

Definition at line 198 of file CoinMpsIO.hpp.

The documentation for this class was generated from the following file:

- /tmp/CoinUtils-2.10.15/CoinUtils/src/CoinMpsIO.hpp